{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":44,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":91,"n_cols":17,"rows_kept":91,"cut":false,"hidden":false,"merged":[[81,15,81,16],[82,15,82,16],[83,15,83,16],[84,15,84,16],[85,15,85,16],[90,1,90,4],[90,5,90,13],[90,15,90,16],[85,5,85,13],[85,1,85,4],[86,0,86,16],[87,1,87,4],[87,5,87,13],[87,15,87,16],[89,5,89,13],[89,15,89,16],[81,1,81,4],[82,1,82,4],[83,1,83,4],[84,1,84,4],[80,5,80,13],[81,5,81,13],[82,5,82,13],[83,5,83,13],[84,5,84,13],[78,0,78,16],[79,1,79,4],[79,5,79,13],[79,15,79,16],[80,1,80,4],[18,15,18,16],[19,15,19,16],[20,15,20,16],[21,15,21,16],[19,1,19,4],[20,1,20,4],[21,1,21,4],[18,5,18,13],[19,5,19,13],[20,5,20,13],[21,5,21,13],[22,1,22,4],[22,5,22,13],[22,15,22,16],[80,15,80,16],[12,1,12,4],[12,5,12,13],[12,15,12,16],[13,1,13,4],[76,1,76,4],[76,5,76,13],[76,15,76,16],[77,1,77,4],[77,5,77,13],[77,15,77,16],[74,1,74,4],[74,5,74,13],[74,15,74,16],[75,1,75,4],[75,5,75,13],[75,15,75,16],[64,1,64,4],[64,5,64,13],[64,15,64,16],[71,0,71,16],[73,1,73,4],[73,5,73,13],[1,1,1,17],[5,0,5,16],[6,0,6,16],[3,0,3,16],[4,0,4,16],[7,0,7,17],[8,0,8,17],[9,0,9,17],[11,0,11,17],[13,5,13,13],[13,15,13,16],[14,1,14,4],[14,5,14,13],[14,15,14,16],[15,1,15,4],[15,5,15,13],[15,15,15,16],[73,15,73,16],[65,1,65,4],[23,0,23,16],[16,0,16,16],[17,1,17,4],[17,5,17,13],[17,15,17,16],[18,1,18,4],[29,1,30,4],[28,5,28,13],[28,15,28,16],[29,5,29,13],[29,15,29,16],[24,1,28,4],[26,5,26,13],[26,15,26,16],[30,5,30,13],[30,15,30,16],[27,5,27,13],[27,15,27,16],[24,5,24,13],[24,15,24,16],[25,5,25,13],[25,15,25,16],[34,5,34,13],[34,15,34,16],[35,5,35,13],[35,15,35,16],[31,5,31,13],[31,15,31,16],[31,1,34,4],[32,5,32,13],[32,15,32,16],[33,5,33,13],[33,15,33,16],[40,1,41,4],[38,5,38,13],[38,15,38,16],[39,5,39,13],[39,15,39,16],[35,1,39,4],[36,5,36,13],[36,15,36,16],[40,5,40,13],[40,15,40,16],[41,5,41,13],[41,15,41,16],[37,5,37,13],[37,15,37,16],[42,5,42,13],[42,15,42,16],[43,5,43,13],[43,15,43,16],[42,1,46,4],[44,5,44,13],[44,15,44,16],[45,5,45,13],[45,15,45,16],[46,5,46,13],[46,15,46,16],[47,5,47,13],[47,15,47,16],[47,1,51,4],[48,5,48,13],[48,15,48,16],[49,5,49,13],[49,15,49,16],[50,5,50,13],[50,15,50,16],[51,5,51,13],[51,15,51,16],[52,5,52,13],[52,15,52,16],[53,5,53,13],[53,15,53,16],[52,1,56,4],[54,5,54,13],[54,15,54,16],[55,5,55,13],[55,15,55,16],[56,5,56,13],[56,15,56,16],[57,5,57,13],[57,15,57,16],[57,1,61,4],[58,5,58,13],[58,15,58,16],[59,5,59,13],[59,15,59,16],[60,5,60,13],[60,15,60,16],[61,5,61,13],[61,15,61,16],[70,1,70,4],[70,5,70,13],[70,15,70,16],[72,1,72,4],[72,5,72,13],[72,15,72,16],[62,1,62,4],[62,5,62,13],[62,15,62,16],[63,1,63,4],[63,5,63,13],[63,15,63,16],[65,5,65,13],[65,15,65,16],[67,1,67,4],[67,5,67,13],[67,15,67,16],[66,0,66,16],[68,1,68,4],[68,5,68,13],[68,15,68,16],[69,1,69,4],[69,5,69,13],[69,15,69,16],[93,0,93,17],[94,0,94,16],[95,0,95,16],[96,0,96,17],[97,0,97,17],[88,1,88,4],[88,5,88,13],[88,15,88,16],[89,1,89,4]]}
[]
[null,"ООО ТД \"Алюминиевые фасады\""]
[]
["Россия, 623100, г. Первоуральск, Свердловская обл., пр. Ильича 30, оф. 5"]
["Тел./факс (3439)64-18-42, 66-64-30"]
["E-mail: tdalfasad@mail.ru"]
["www.алфасад.рф"]
[]
[]
["Комплектующие  системы Алкон-2 "]
[]
["Направляющие (композит)"]
["№","Эскиз",null,null,null,"Наименование",null,null,null,null,null,null,null,null,"Ед.","Обозначение"]
["1",null,null,null,null,"Стойка С-направляющая",null,null,null,null,null,null,null,null,"м.п.","НПВФ 447",10400]
["2",null,null,null,null,"Стойка С-направляющая безопорная",null,null,null,null,null,null,null,null,"м.п.","НПВФ 446",10401]
["3",null,null,null,null,"Стойка С-направляющая эконом",null,null,null,null,null,null,null,null,"м.п.","НПВФ 444",10402]
["Направляющие (керамогранит)"]
[4,null,null,null,null,"Стойка Т-направляющая паз",null,null,null,null,null,null,null,null,"м.п.","НПВФ 01"]
[5,null,null,null,null,"Стойка Г-направляющая паз",null,null,null,null,null,null,null,null,"м.п.","НПВФ 02"]
[6,null,null,null,null,"Стойка Т-направляющая 80х70",null,null,null,null,null,null,null,null,"м.п.","НПВФ 440"]
[7,null,null,null,null,"Стойка Т-направляющая 70х60",null,null,null,null,null,null,null,null,"м.п.","НПВФ 443"]
[8,null,null,null,null,"Стойка Г-направляющая 40х70",null,null,null,null,null,null,null,null,"м.п.","НПВФ 441"]
[9,null,null,null,null,"Горизонтальная направляющая",null,null,null,null,null,null,null,null,"м.п.","НПВФ 442"]
["Кронштейны"]
[10,null,null,null,null,"Кронштейн несущий КН-70 (лёгкого фасада)",null,null,null,null,null,null,null,null,"шт.","НПВФ 20",0]
[11,null,null,null,null,"Кронштейн несущий КН-100",null,null,null,null,null,null,null,null,"шт.","НПВФ 13",1]
[12,null,null,null,null,"Кронштейн несущий КН-160",null,null,null,null,null,null,null,null,"шт.","НПВФ 36",2]
[13,null,null,null,null,"Кронштейн несущий КН-190",null,null,null,null,null,null,null,null,"шт.","НПВФ 61",3]
[14,null,null,null,null,"Кронштейн несущий КН-220",null,null,null,null,null,null,null,null,"шт.","НПВФ 64",4]
[15,null,null,null,null,"Кронштейн усиленный КУ-100",null,null,null,null,null,null,null,null,"шт.","НПВФ 37",5]
[16,null,null,null,null,"Кронштейн усиленный КУ-160",null,null,null,null,null,null,null,null,"шт.","НПВФ 38",6]
[17,null,null,null,null,"Кронштейн усиленный с прищепкой КУП-100",null,null,null,null,null,null,null,null,"шт.","НПВФ 57",7]
[18,null,null,null,null,"Кронштейн усиленный с прищепкой КУП-160",null,null,null,null,null,null,null,null,"шт.","НПВФ 58",8]
[19,null,null,null,null,"Кронштейн усиленный с прищепкой КУП-190",null,null,null,null,null,null,null,null,"шт.","НПВФ 62",9]
[20,null,null,null,null,"Кронштейн усиленный с прищепкой КУП-220",null,null,null,null,null,null,null,null,"шт.","НПВФ 65",10]
[21,null,null,null,null,"Кронштейн опорный КО-70 (лёгкого фасады)",null,null,null,null,null,null,null,null,"шт.","НПВФ 21",11]
[22,null,null,null,null,"Кронштейн опорный КО-100",null,null,null,null,null,null,null,null,"шт.","НПВФ 15",12]
[23,null,null,null,null,"Кронштейн опорный КО-160",null,null,null,null,null,null,null,null,"шт.","НПВФ 53",13]
[24,null,null,null,null,"Кронштейн опорный КО-190",null,null,null,null,null,null,null,null,"шт.","НПВФ 60",14]
[25,null,null,null,null,"Кронштейн опорный КО-220",null,null,null,null,null,null,null,null,"шт.","НПВФ 63",15]
[26,null,null,null,null,"Кронштейн опорный КО-100",null,null,null,null,null,null,null,null,"шт.","НПВФ 14",16]
[27,null,null,null,null,"Кронштейн опорный КО-160",null,null,null,null,null,null,null,null,"шт.","НПВФ 54",17]
[28,null,null,null,null,"Кронштейн доборный несущий КДН-90",null,null,null,null,null,null,null,null,"шт.","НПВФ 16-90",18]
[29,null,null,null,null,"Кронштейн доборный несущий КДН-110",null,null,null,null,null,null,null,null,"шт.","НПВФ 16-110",19]
[30,null,null,null,null,"Кронштейн доборный несущий КДН-140",null,null,null,null,null,null,null,null,"шт.","НПВФ 16-140",20]
[31,null,null,null,null,"Кронштейн доборный несущий КДН-170",null,null,null,null,null,null,null,null,"шт.","НПВФ 16-170",21]
[32,null,null,null,null,"Кронштейн доборный несущий КДН-220",null,null,null,null,null,null,null,null,"шт.","НПВФ 16-220",22]
[33,null,null,null,null,"Кронштейн доборный усиленный КДУ-90",null,null,null,null,null,null,null,null,"шт.","НПВФ 55-90",23]
[34,null,null,null,null,"Кронштейн доборный усиленный КДУ-110",null,null,null,null,null,null,null,null,"шт.","НПВФ 55-110",24]
[35,null,null,null,null,"Кронштейн доборный усиленный КДУ-140",null,null,null,null,null,null,null,null,"шт.","НПВФ 55-140",25]
[36,null,null,null,null,"Кронштейн доборный усиленный КДУ-170",null,null,null,null,null,null,null,null,"шт.","НПВФ 55-170",26]
[37,null,null,null,null,"Кронштейн доборный усиленный КДУ-220",null,null,null,null,null,null,null,null,"шт.","НПВФ 55-220",27]
[38,null,null,null,null,"Кронштейн доборный опорный КДО-90",null,null,null,null,null,null,null,null,"шт.","НПВФ 17-90",28]
[39,null,null,null,null,"Кронштейн доборный опорный КДО-110",null,null,null,null,null,null,null,null,"шт.","НПВФ 17-110",29]
[40,null,null,null,null,"Кронштейн доборный опорный КДО-140",null,null,null,null,null,null,null,null,"шт.","НПВФ 17-140",30]
[41,null,null,null,null,"Кронштейн доборный опорный КДО-170",null,null,null,null,null,null,null,null,"шт.","НПВФ 17-170",31]
[42,null,null,null,null,"Кронштейн доборный опорный КДО-220",null,null,null,null,null,null,null,null,"шт.","НПВФ 17-220",32]
[43,null,null,null,null,"Кронштейн доборный усиленный с прищепкой КДУП-90",null,null,null,null,null,null,null,null,"шт.","НПВФ 56-90",33]
[44,null,null,null,null,"Кронштейн доборный усиленный с прищепкой КДУП-110",null,null,null,null,null,null,null,null,"шт.","НПВФ 56-110",34]
[45,null,null,null,null,"Кронштейн доборный усиленный с прищепкой КДУП-140",null,null,null,null,null,null,null,null,"шт.","НПВФ 56-140",35]
[46,null,null,null,null,"Кронштейн доборный усиленный с прищепкой КДУП-170",null,null,null,null,null,null,null,null,"шт.","НПВФ 56-170",36]
[47,null,null,null,null,"Кронштейн доборный усиленный с прищепкой КДУП-220",null,null,null,null,null,null,null,null,"шт.","НПВФ 56-220",37]
[48,null,null,null,null,"Вынос угловой несущий ВУН-500",null,null,null,null,null,null,null,null,"шт.","НПВФ 42",38]
[49,null,null,null,null,"Вынос угловой опорный ВУО-500",null,null,null,null,null,null,null,null,"шт.","НПВФ 44",39]
[50,null,null,null,null,"Угловой соединитель УС-100",null,null,null,null,null,null,null,null,"шт.","НПВФ 41",40]
[51,null,null,null,null,"Угловой соединитель УС-70",null,null,null,null,null,null,null,null,"шт.","НПВФ 43",400]
["Крепёж обрамлений, соединений"]
[52,null,null,null,null,"Уголок 70х40 L=30",null,null,null,null,null,null,null,null,"шт.","НПВФ 28",400]
[53,null,null,null,null,"Уголок 20х20",null,null,null,null,null,null,null,null,"п/м.","НПВФ 27",401]
[54,null,null,null,null,"Соединитель L=130",null,null,null,null,null,null,null,null,"шт.","НПВФ 30",402]
[55,null,null,null,null,"F-профиль",null,null,null,null,null,null,null,null,"п/м.","НПВФ 457",403]
["Элементы крепления облицовки (композит)"]
[56,null,null,null,null,"Зацеп кассетный",null,null,null,null,null,null,null,null,"шт.","НПВФ 09",400]
[57,null,null,null,null,"Зацеп кассетный с винтом",null,null,null,null,null,null,null,null,"шт.","НПВФ 50",401]
[58,null,null,null,null,"Зацеп кассетный эконом",null,null,null,null,null,null,null,null,"шт.","НПВФ 51",402]
[59,null,null,null,null,"Зацеп кассетный эконом с винтом",null,null,null,null,null,null,null,null,"шт.","НПВФ 52",403]
[60,null,null,null,null,"Икля под зацеп (левая/правая)",null,null,null,null,null,null,null,null,"шт.","НПВФ 10/11",404]
[61,null,null,null,null,"Усилитель кассет угловой",null,null,null,null,null,null,null,null,"шт.","НПВФ 457",405]
["Элементы крепления облицовки (керамогранит)"]
[62,null,null,null,null,"Планка дистанционная в паз",null,null,null,null,null,null,null,null,"шт.","НПВФ 07"]
[63,null,null,null,null,"Кляммер рядовой (нерж) в паз",null,null,null,null,null,null,null,null,"шт.","НПВФ 08"]
[64,null,null,null,null,"Кляммер нижний (нерж) в паз",null,null,null,null,null,null,null,null,"шт.","НПВФ 25"]
[65,null,null,null,null,"Кляммер рядовой (нерж) краб",null,null,null,null,null,null,null,null,"шт.","НПВФ 46"]
[66,null,null,null,null,"Кляммер стартовый (нерж)",null,null,null,null,null,null,null,null,"шт.","НПВФ 47"]
[67,null,null,null,null,"Кляммер боковой (нерж)",null,null,null,null,null,null,null,null,"шт.","НПВФ 48"]
[68,null,null,null,null,"Кляммер угловой (нерж)",null,null,null,null,null,null,null,null,"шт.","НПВФ 49"]
["Дополнительные элементы"]
[69,null,null,null,null,"Прокладка паронитовая ППН-100",null,null,null,null,null,null,null,null,"шт.","НПВФ 31"]
[70,null,null,null,null,"Прокладка паронитовая ППО-100",null,null,null,null,null,null,null,null,"шт.","НПВФ 32"]
[71,null,null,null,null,"Прокладка паронитовая ППУ-100",null,null,null,null,null,null,null,null,"шт.","НПВФ 59"]
[72,null,null,null,null,"Уплотнитель 0100 в паз",null,null,null,null,null,null,null,null,"шт.","УК 0100"]